12/2/2020 CH

Converting MFT Firmware

**Updating the firmware on the Multi-Function Thermometer (MFT)**

Download the Blue2 Reader app (from the App store or Google Play) and install it on your mobile device.

Turn on Bluetooth on your mobile device.

Ensure Internet access is available and follow these steps to download firmware updates.

1. Launch Blue2 Reader app

2. Tap Scan on the Blue2 Reader app

3. Turn on the MFT – it will begin to blink green

4. The MFT will display in the list of available devices on the Blue2 Reader app

5. Tap the MFT in the list of devices to connect with it – it will blink blue once connected

6. On the Blue2 Reader app, tap Firmware Update

7. On the Firmware Update page, tap Check for Updates

8. The latest available firmware will be listed

9. Tap the latest available firmware

10. The app will send the new firmware to the MFT

**Converting the firmware on the Multi-Function Thermometer (MFT)**

Download the Blue2 Reader app (from the App store or Google Play) and install it on your mobile device. Ensure Internet access is available and follow these steps to download firmware updates.

Turn on Bluetooth on your mobile device.

1. Launch Blue2 Reader app

2. Tap Scan on the Blue2 Reader app

3. Turn on the MFT – it will begin to blink green

4. The MFT will display in the list of available devices on the Blue2 Reader app

5. Tap the MFT in the list of devices to connect with it – it will blink blue once connected

6. On the Blue2 Reader app, tap Firmware Update

7. Tap Custom updates toggle

8. Type “convert” (without the quotes) in the field over the gray directory

9. On the Firmware Update page, tap Check for Updates - All firmware versions (McD and Standard) available (latest and previous) will be listed

10. Tap the latest available firmware in the version you want

11. The app will send the new firmware to the MFT